**Powerx 3ltr Multi Use Foam Extinguisher Data Sheet**

|  |  |
| --- | --- |
| OUR PN | 81/03693 |
| Capacity (ltr) | 3Ltr |
| Fire Rating | 13A 70B 40F |
| Height | 455mm |
| Cylinder Diameter (mm) | 130mm |
| Overall Width (mm) | 217mm |
| Filled Weight (kg) | 5.3kg |
| Range of Throw (m) | >5 |
| Duration of Discharge (secs) | 13 |
| Working Pressure (at 20°C) | 12 |
| Temperature Range (°C) | +5°C to +60°C |
| BS EN3 Approved | Yes |
| MED Approved | No |
| 35KV | Yes |
| Pressure Relief Valve | Yes |
| Low Freeze Additive | No |
| Part Number | 81/03693 |
| Model Number | F3K |