**Powerx 3ltr Multi Use Foam Extinguisher Data Sheet**

|  |  |
| --- | --- |
| OUR PN  | 81/03693 |
| Capacity (ltr)   | 3Ltr |
| Fire Rating   | 13A 70B 40F |
| Height    | 455mm |
| Cylinder Diameter (mm)  | 130mm |
| Overall Width (mm)    | 217mm |
| Filled Weight (kg)    | 5.3kg |
| Range of Throw (m)   | >5 |
| Duration of Discharge (secs)  | 13 |
| Working Pressure (at 20°C)   | 12 |
| Temperature Range (°C)   | +5°C to +60°C |
| BS EN3 Approved    | Yes |
| MED Approved   | No |
| 35KV | Yes |
| Pressure Relief Valve | Yes |
| Low Freeze Additive | No |
| Part Number   | 81/03693 |
| Model Number    | F3K |